ཆུ་འཐག གཞི་རྟེན་དགོས་ཚད། གོ་རིམ ༡ པ།

**BHUTAN STANDARD**

**Rice Mill – Basic Requirements (Part 1)**



ICS 65.060.10

© Copyright 2018

**BHUTAN STANDARDS BUREAU**

The National Standards Body of Bhutan

THIMPHU 11001

ཆུ་འཐག གཞི་རྟེན་དགོས་ཚད། གོ་རིམ ༡ པ།

**BHUTAN STANDARD**

**Rice Mill – Basic Requirements (Part 1)**

**PDF disclaimer**

This PDF file may contain embedded typefaces. In accordance with Adobe’s Licensing policy, this file

may be printed or viewed but shall not be edited unless the typefaces which are embedded are licensed to and installed on the computer performing editing. In downloading this file, parties accept therein the responsibility of not infringing Adobe’s licensing policy. The Bhutan Standards Bureau accepts no liability in this area.

Adobe is a trademark of Adobe Systems Incorporated.

**COPYRIGHT PROTECTED DOCUMENT**

© BSB 2018

All rights reserved. Unless otherwise specified, no part of this publication may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm,

without permission in writing from either BSB at the address below in the country of the requester.

Director General

Bhutan Standards Bureau

Thimphu-11001

Tel : 00975-2-325104/325401

Fax: 00975-2-323712/328298

Web: [www.bsb.gov.bt](http://www.bsb.gov.bt/)

Published in xxxxxxx 2018

Contents

[FOREWORD iv](#_Toc526419546)

[1 Scope 1](#_Toc526419547)

[2 Normative References 1](#_Toc526419548)

[3 Definitions 1](#_Toc526419549)

[3.1 Rice Mill 1](#_Toc526419550)

[3.2 De-Husker 1](#_Toc526419551)

[3.3 Polisher 1](#_Toc526419552)

[3.4 Combined Types 1](#_Toc526419553)

[3.5. Milled Rice 1](#_Toc526419554)

[3.6 Food Grade Material 1](#_Toc526419555)

[3.7. Milling recovery index 1](#_Toc526419556)

[3.8 Head Rice recovery index 2](#_Toc526419557)

[3.9 Rough Rice or Paddy 2](#_Toc526419558)

[4 The general standard for Rice Mill shall cover; 2](#_Toc526419559)

[4.1 Safety requirements 2](#_Toc526419560)

[4.3 Requirement of Operational performance 2](#_Toc526419561)

[4.4 Test Sample 2](#_Toc526419562)

[Annex A (Normative) 3](#_Toc526419563)

[Bibliography 4](#_Toc526419564)

# FOREWORD

This Bhutan Standards for Power Tillers–Test Code (Part 2) was adopted by Bhutan Standards Bureau after the draft finalization by the Mechanical Engineering Technical Committee and endorsed by BSB Board.

ཆུ་འཐག གཞི་རྟེན་དགོས་ཚད། གོ་རིམ ༡ པ།

**BHUTAN STANDARD**

**Rice Mill – Basic Requirements (Part 1)**

# 1 Scope

This standard specifies the general requirements for Rice Mill and shall apply to De husker, Polisher and Combined types. It excludes the test methods of Rice Mill.

# 2 Normative References

There are no normative reference for this document

# 3 Definitions

For the purposes of this standard, the following definitions apply.

## 3.1 Rice Mill

A machine or equipment used for converting rough rice to milled rice.

## 3.2 De-Husker

A machine which is used to removes the husk from the rough rice.

## 3.3 Polisher

A machine used for polishing kernels of rice to change their appearance, taste and texture.

## 3.4 Combined Types

A machine which can perform both the operations of de-husking and polishing

## 3.5. Milled Rice

The white grain or kernel comprising the endosperm and the seed left after removal of husk.

## 3.6 Food Grade Material

Any material when it comes in contact with food does not contaminate the food beyond the limit of prohibited substances given in annex A, table 1.

## 3.7. Milling recovery index

It is the ratio of milling recovery rate of tested machine and the laboratory test reference value.

## 3.8 Head Rice recovery index

It is the ratio of head rice recovery rate of tested machine and the laboratory test reference value.

## 3.9 Rough Rice or Paddy

It is un-hulled or un-husked rice (Oryza *sativa*)

# 4 The general standard for Rice Mill shall cover;

**4.1** Safety Requirements

**4.2** Structure Requirements

**4.3** Requirement of Operational Performance

**4.4** Test Sample

## 4.1 Safety requirements

**4.1.1** There shall be safety guard for moving parts which are prone to injury and guard shall be placed in between the moving parts and operator at appropriate safe distance.

**4.1.2** The guard shall have enough strength and durability under the normal operational condition and the guard which does not require to be removed, should be firmly fixed on the machine.

**4.1.3** Parts that come in contact with the rough rice should be made of food grade material.

**4.1.4** The machine shall be equipped with Instruction and operation manuals.

**4.2 Structure requirements**

**4.2.1** The main components shall not be abnormal or broken.

**4.2.2** The operator should not have difficulty in operating and controlling the components.

**4.2.3** There should not be any defects that may affect the operator.

**4.2.4** The food grade materials for processing machine shall be as given in annex A, Table 2

## 4.3 Requirement of Operational performance

**4.3.1** Milling recovery index should not be lower than 0.9.

**4.3.2** Head rice recovery index should not be lower than 0.75.

**4.3.3** The noise level for rice mill should not exceed 100dBA for 2 hours of continuous operation.

## 4.4 Test Sample

The test sample shall be new machine and it shall be adjusted as per the manufacturer’s specification.

# Annex A (Normative)

*(Clause 3.6 and 4.2.4)*

Presence of any traces of prohibited substance should be within the limit prescribed in Table 1.

**Table 1** Prohibited substances in food contact parts.

|  |  |  |
| --- | --- | --- |
| **Sl. No** | **Elements** | **Limit Value** |
| 1. | Lead (Pb) | < 0.1% |
| 2. | **Antimony (Sb)** | < 5 % |
| 3. | Cadmium (Cd) | < 0.01 – 0.04 % |
| 4. | Mercury (Hg) | < 0.1 % |
| 5. | Cyanide | 0 |

**Table 2** Recommended food grade materials for different operating conditions:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sl. No** | **Metal Type** | **Operating Condition** | | | | **Food Contact Parts** |
| **Wet** | | | **Dry** |
| **Acid**  **(pH 0-6)** | **Neutral**  **(pH 6-8)** | **Alkaline**  **(pH 8-14)** |
| 1. | Carbon Steel | Not Recommended | Recommended with Coating/Plating | Recommended with Coating/Plating | Recommended | Hopper, Shaft, Outer body |
| 2. | Stainless Steel (SS) | SS 304, Recommended | SS304 Recommended | SS304 Recommended | SS200, Recommended | Shaft, Screen, Outlet |
| 3. | Cast Iron | Not Recommended | Not Recommended | Not Recommended | Recommended with coating/Plating | Outer Body |

# Bibliography

1. ISO: 3971-1977 (E/F) Rice Milling – Symbols and Equivalent Terms
2. ISO Recommendation R712: 1968 Determinations of Moisture Content Routine Method, International Organization for Standardization.
3. AMTEC Standard: 1989 Rice Mill – Methods of Test, Draft Standard: Agricultural Machinery

Testing and Evaluation Centre, University of the Philippines at Los Banos, Philippines.

1. ASAE Standard: ASAES352, 1977 Moisture measurement – Grain and Seeds, American Society of Agricultural Engineers, St. Joseph, Michigan, USA
2. Agricultural Mechanization Institute: 1989 Diagrams of Large-Scale and Small-Scale Rice Milling

Systems in the Republic of Korea.

1. Regional Network for Agricultural Machinery (RNAM): 1995 Test Codes and Procedures for Farm Machinery, Technical Series No. 12

**Mechanical Engineering Technical Committee (TC-08)**

***Organization Representatives***

**Chairman**

Agriculture Machinery Centre, Mr. Chetem Wangchen

Ministry of Agriculture and Forest

**Members**

Agriculture Machinery Centre, Mr. Kinga Norbu

Ministry of Agriculture and Forest

Agriculture Machinery Centre, Mr. Sangay Lhendup

Ministry of Agriculture and Forest

Construction Development Corporation Limited Mr. Karma Loday

Farm Machinery Corporation Limited, Ministry of Finance Mr. Karma Thinley

Department of Agriculture, Mr. Tirtha Bdr. Katwal

Ministry of Agriculture and Forest

Road Safety and Transport Authority, Mr. Phuntsho Wangdi

Ministry of Information and Communication

Technical Training Institute, Samthang, Mr. Sangay Wangchuk

Ministry of Labour and Human Resources

Bhutan Standards Bureau Mr. Sonam Phuntsho, Director General

(Ex- Officio member)

**Member Secretary**

Pelden Dendup Standardization Division Bhutan Standards Bureau