**སྲིབ་རྡུང་འཕྲུལ་ཆས། གཞི་རྟེན་དགོས་ཚད། གོ་རིམ ༡ པ།**

**BHUTAN STANDARD**

**Cereal Flaking Machine: Basic Requirements (Part 1)**



ICS 65.060.10

© Copyright 2018

**BHUTAN STANDARDS BUREAU**

The National Standards Body of Bhutan

THIMPHU 11001

**སྲིབ་རྡུང་འཕྲུལ་ཆས། གཞི་རྟེན་དགོས་ཚད། གོ་རིམ ༡ པ།**

**BHUTAN STANDARD**

**Cereal Flaking Machine: Basic Requirements (Part 1)**

**PDF disclaimer**

This PDF file may contain embedded typefaces. In accordance with Adobe’s Licensing policy, this file

may be printed or viewed but shall not be edited unless the typefaces which are embedded are licensed to and installed on the computer performing editing. In downloading this file, parties accept therein the responsibility of not infringing Adobe’s licensing policy. The Bhutan Standards Bureau accepts no liability in this area.

Adobe is a trademark of Adobe Systems Incorporated.

**COPYRIGHT PROTECTED DOCUMENT**

© BSB 2018

All rights reserved. Unless otherwise specified, no part of this publication may be reproduced orutilized in any form or by any means, electronic or mechanical, including photocopying and microfilm,

without permission in writing from either BSB at the address below in the country of the requester.

Director General

Bhutan Standards Bureau

Thimphu-11001

Tel : 00975-2-325104/325401

Fax: 00975-2-323712/328298

Web: [www.bsb.gov.bt](http://www.bsb.gov.bt/)

Published in October 2018

Contents

[FOREWORD iv](#_Toc526791694)

[1 Scope 1](#_Toc526791695)

[2 Normative Reference 1](#_Toc526791696)

[3 Definition 1](#_Toc526791697)

[3.1 Cereal Flaking machine 1](#_Toc526791698)

[3.2 Cereal 1](#_Toc526791699)

[3.3 Flaking 1](#_Toc526791700)

[3.4 Food grade material 1](#_Toc526791701)

[3.5 Flaking recovery rate 1](#_Toc526791702)

[3.6 Flaking recovery index 1](#_Toc526791703)

[3.7 Flaking Capacity 1](#_Toc526791704)

[4 General Requirement of the cereal flaking machine shall cover; 1](#_Toc526791705)

[4.1. Safety requirements 2](#_Toc526791706)

[4.2. Requirements of operational performance 2](#_Toc526791707)

[4.3. Structure requirements 2](#_Toc526791708)

[5 Test Sample 2](#_Toc526791709)

[Annex A (Normative) 3](#_Toc526791710)

[Bibliography 4](#_Toc526791711)

# FOREWORD

This Bhutan Standards for Power Tillers–Test Code (Part 2) was adopted by Bhutan Standards Bureau after the draft finalization by the Mechanical Engineering Technical Committee and endorsed by BSB Board.

**སྲིབ་རྡུང་འཕྲུལ་ཆས། གཞི་རྟེན་དགོས་ཚད། གོ་རིམ ༡ པ།**

**BHUTAN STANDARD**

**Cereal Flaking Machine: Basic Requirements (Part 1)**

# Scope

This standard specifies the basic requirements for the cereal flaking machines.

# Normative Reference

There are no normative references for this document.

# Definition

## 3.1 Cereal Flaking machine

A machine used for flattening the cereals mainly rice and maize.

## 3.2 Cereal

Are generally of the gramineous family refers to crop harvested for dry grain only.

## 3.3 Flaking

It is a processing technique by which whole grains of cereals are normally processed before being used as an ingredient to produce a range of products such as rice flakes and cornflakes.

## 3.4 Food grade material

Any material when it comes in contact with food does not contaminate the food beyond the limit of prohibited substances given in annex A, Table 1.

## 3.5 Flaking recovery rate

The percentage output of flakes in relation to the total input of roasted cereal in a tested machine.

## 3.6 Flaking recovery index

It is the ratio of recovery rate of tested machine to that of manual pounding.

## 3.7 Flaking Capacity

It is the weight of the input cereal processed by the test machine over a time period.

# General Requirement of the cereal flaking machine shall cover;

4.1. Safety Requirements

4.2. Requirement of Operational Performance

4.4. Structure Requirements

## 4.1. Safety requirements

4.1.1. There shall be safety guard for moving parts which are prone to injury and guard shall be placed in between the moving parts and operator.

4.1.2. The guard shall have enough strength and durability under the normal operational condition and the guard which does not require to be removed or should be firmly fixed on the machine.

4.1.3. All safety symbols and labels shall be illustrated and clearly visiable to operator.

4.1.4. Parts that come in contact with the flake should be of food grade materials.

4.1.5. The machine should be fitted with the mechanism to remove the finished products.

4.1.6. There should not be any defects that may affect the operator.

4.1.7. The machine shall be equipped with instruction and operation mannuals.

## 4.2. Requirements of operational performance

4.2.1. Flaking recovery index should be equal to 1.0 or above.

4.2.2 Flaking capacity should be as specified by the manufacturer.

4.2.2. Flaking operation should be smoothly conducted.

4.2.4. The noise level for flaking machine should not exceed 100dB (A) for 2 hours of continuous operation.

## 4.3. Structure requirements

4.3.1. The main components shall not be abnormal or broken.

4.3.2.The operator should not have difficulty in operating and controlling the components.

4.3.3The food grade materials for processing machine shall be as given in annex A, Table 2

# Test Sample

The test sample shall be a new machine and it shall be adjusted as per the manufacturer’s specification.

# Annex A (Normative)

*(Clause 3.4 and 4.3.3)*

Presence of any traces of prohibited substance should be within the limit prescribed in Table 1.

**Table 1** Prohibited substances in food contact parts.

|  |  |  |
| --- | --- | --- |
| **Sl. No** | **Elements** | **Limit Value** |
| 1. | Lead (Pb) | < 0.1% |
| 2. | **Antimony (Sb)** | < 5 % |
| 3. | Cadmium (Cd) | < 0.01 – 0.04 % |
| 4. | Mercury (Hg) | < 0.1 % |
| 5. | Cyanide | 0 |

**Table 2** Recommended food grade materials for different operating conditions

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Sl. No** | **Metal Type** | **Operating Condition** | | | | **Food Contact Parts** |
| **Wet** | | | **Dry** |
| **Acid (pH 0-6)** | **Neutral (pH 6-8)** | **Alkaline (pH 8-14)** |
| 1. | Carbon Steel | Not Recommended | Recommended with Coating/Plating | Recommended with Coating/Plating | Recommended | Hopper, Shaft, Outer body |
| 2. | Stainless Steel (SS) | SS 304, Recommended | SS304 Recommended | SS304 Recommended | SS200, Recommended | Shaft, Screen, Outlet |
| 3. | Cast Iron | Not Recommended | Not Recommended | Not Recommended | Recommended with coating/Plating | Outer Body |

# Bibliography

1. ISO Recommendation R712: 1988 Deternination of Moisture Content Routine Method
2. ASAE Standard: ASAES352, 1977 Moisture measurement – Grain and Seeds, American Society of Agricultural Engineers, St. Joseph, Michigan, USA
3. AMTEC Standard: 1989 Rice Mill – Methods of Test, Draft Standard: Agricultural Machinery Testing and Evaluation Centre, University of the Philippines at Los Banos, Philippines.
4. Regional Network for Agricultural Machinery (RNAM): 1995 Test Codes and Procedures for Farm Machinery, Technical Series No. 12

**Mechanical Engineering Technical Committee (TC-08)**

***Organization Representatives***

**Chairman**

Agriculture Machinery Centre, Mr. Chetem Wangchen

Ministry of Agriculture and Forest

**Members**

Agriculture Machinery Centre, Mr. Kinga Norbu

Ministry of Agriculture and Forest

Agriculture Machinery Centre, Mr. Sangay Lhendup

Ministry of Agriculture and Forest

Construction Development Corporation Limited Mr. Karma Loday

Farm Machinery Corporation Limited, Ministry of Finance Mr. Karma Thinley

Department of Agriculture, Mr. Tirtha Bdr. Katwal

Ministry of Agriculture and Forest

Road Safety and Transport Authority, Mr. Phuntsho Wangdi

Ministry of Information and Communication

Technical Training Institute, Samthang, Mr. Sangay Wangchuk

Ministry of Labour and Human Resources

Bhutan Standards Bureau Mr. Sonam Phuntsho, Director General

(Ex- Officio member)

**Member Secretary**

Pelden Dendup

Standardization Division

Bhutan Standards Bureau