**སྲིབ་རྡུང་འཕྲུལ་ཆས། བརྟག་དཔྱད་སྒྲིག་ལུགས། གོ་རིམ ༢ པ།**

**BHUTAN STANDARD**

**Cereal Flaking Machine- Test Code (Part 2)**



ICS 65.060.10

© Copyright 2018

**BHUTAN STANDARDS BUREAU**

The National Standards Body of Bhutan

THIMPHU 11001

**སྲིབ་རྡུང་འཕྲུལ་ཆས། བརྟག་དཔྱད་སྒྲིག་ལུགས། གོ་རིམ ༢ པ།**

**BHUTAN STANDARD**

**Cereal Flaking Machine- Test Code (Part 2)**

**PDF disclaimer**

This PDF file may contain embedded typefaces. In accordance with Adobe’s Licensing policy, this file may be printed or viewed but shall not be edited unless the typefaces which are embedded are licensed to and installed on the computer performing editing. In downloading this file, parties accept therein the responsibility of not infringing Adobe’s licensing policy. The Bhutan Standards Bureau accepts no liability in this area.

Adobe is a trademark of Adobe Systems Incorporated.

**COPYRIGHT PROTECTED DOCUMENT**

© BSB 2018

All rights reserved. Unless otherwise specified, no part of this publication may be reproduced or utilized in any form or by any means, electronic or mechanical, including photocopying and microfilm,

without permission in writing from either BSB at the address below in the country of the requester.

Director General

Bhutan Standards Bureau

Thimphu-11001

Tel : 00975-2-325104/325401

Fax: 00975-2-323712/328298

Web: www.bsb.gov.bt

Published in October 2018

Contents

[FOREWORD iv](#_Toc526773307)

[1 Scope 1](#_Toc526773308)

[2 Normative Reference 1](#_Toc526773309)

[3 Definitions 1](#_Toc526773310)

[3.1 Flaking time 1](#_Toc526773311)

[3.2 Others 1](#_Toc526773312)

[3.3 Flake 1](#_Toc526773313)

[4 General conditions of the test 1](#_Toc526773314)

[5 Test items and methods 1](#_Toc526773315)

[5.1 Verification of structure 1](#_Toc526773316)

[5.2 Safety test 2](#_Toc526773317)

[5.3 Operation test 2](#_Toc526773318)

[5.3.1 The items to be measured or investigated are; 2](#_Toc526773319)

[6 Formulae 2](#_Toc526773320)

[6.1 Flaking Recovery Rate 2](#_Toc526773321)

[6.2 Flaking Recovery Index 3](#_Toc526773322)

[6.3 Flaking Capacity 3](#_Toc526773323)

[7. Inspection after disassembling 3](#_Toc526773324)

[Annexure A (Normative) 4](#_Toc526773325)

[Bibliography 5](#_Toc526773326)

#

# FOREWORD

This Bhutan Standards for Power Tillers–Test Code (Part 2) was adopted by Bhutan Standards Bureau after the draft finalization by the Mechanical Engineering Technical Committee and endorsed by BSB Board

**སྲིབ་རྡུང་འཕྲུལ་ཆས། བརྟག་དཔྱད་སྒྲིག་ལུགས། གོ་རིམ ༢ པ།**

**BHUTAN STANDARD**

**Cereal Flaking Machine- Test Code (Part 2)**

# Scope

 This test code specifies the test methods for cereal flaking machines.

# Normative Reference

There are no normative references for this document

# Definitions

For the purpose of this document, the definitions have given in the standard of cereal flaking machines, BTS March, 2017.

## 3.1 Flaking time

It is a time taken to convert the input cereal to flakes by the flaking machine.

## 3.2 Others

Any additional verifications that may be required to be undertaken for enhancing the precision of any test items.

## 3.3 Flake

The final product that is retained on the sieve size of 5mm for maize flake and 3 mm for rice flake.

# General conditions of the test

* 1. The cereal flaking machine subjected to the test shall be run as per the manufacture’s indication and specifications.
	2. The cereal flaking machine subjected to the test shall be well adjusted and prepared as per the requirements and the manufacturer’s indication.
	3. The prime mover used for the tests shall be selected from those indicated by the manufacturer.
	4. All measuring instruments used for the test shall be calibrated with relevant agencies or certification body.

# Test items and methods

## 5.1 Verification of structure

The objective of this test is to confirm the specifications of a cereal flaking machine given by the manufacturer. The items to be verified are as per the Annex A.

## 5.2 Safety test

The objective of this test is to ascertain the safety features of the cereal flaking machine. It shall be performed by;

1. Verifying safety devices
2. Inspection of the caution labels
3. Availability of instruction and operation manuals.
4. Others

## 5.3 Operation test

The objective of this test is to assess the flaking recovery rate, flaking recovery index, flaking capacity and handling. To carry out these tests, following conditions shall be maintained;

1. The manufacturer’s specification and instruction or operation manual shall be followed for fitting the accessories and any other adjustments.
2. The cereal flaking machine shall be operated by at least two experienced operators.
3. The manual pounding will be used to determine the reference value for estimating flaking recovery index.
4. Flaking recovery index will be estimated to assess the efficiency of the flaking cereal crops.

### 5.3.1 The items to be measured or investigated are;

1. Test condition of cereal
2. Mechanical condition of the cereal flaking machine
3. Operating condition of cereal flaking machine
4. Flaking recovery
5. Flaking capacity
6. Energy consumption
7. Ease of handling
8. Noise level
9. Others

# 6 Formulae

The flaking recovery rate, flaking recovery index and flaking capacity shall be calculated as follows;

## 6.1 Flaking Recovery Rate

Where:

FR= Flaking recovery (%) by machine

W1= Weight of roasted cereal (kg)

W2= Weight of flake (kg)

Where:

FRR= Flaking recovery for reference (%) by manual

W1 = Weight of roasted cereal (kg)

W2= Weight of flake (kg)

## 6.2 **Flaking Recovery Index**

Where:

FRI: Flaking recovery index

FRR: Flaking recovery for reference by manual

FR: Flaking recovery by machine

## 6.3 Flaking Capacity

Where:

CF: Flaking capacity (kg/h)

W: Weight of input sample after roasting (kg)

TF: Flaking time (h)

# 7. Inspection after disassembling

If any abnormalities are observed during any of the above tests, causes may be investigated by disassembling the specific parts.

#

# Annexure A (Normative)

**SPECIFICATION SHEET FOR CEREAL FLAKING MACHINE**

**A Corn flake machine**

1. Model:
2. Make:
3. Type :
4. Serial number:
5. Overall dimensions
6. Length:
7. Width:
8. Height:

**B Prime Mover**

1. Power source:
2. Type:
3. Make:
4. Rated power :
5. Type of starter:
6. Type of fuel:
7. Others
8. Diameter of driving pulley:
9. Diameter of main shaft pulley:
10. Diameter of sieve hole:
11. Diameter of flaking chamber:
12. Diameter of main shaft:

**C. Roller**

1. Thickness:
2. Diameter:

**D. Adjustable range of drum and roller:**

**Note: All dimensions in millimeters (mm)**

#

# Bibliography

Design and development of a small/ medium scale rice flaking machinery for manufacture of rice flake

**Mechanical Engineering Technical Committee (TC-08)**

|  |  |
| --- | --- |
| ***Organization***  | ***Representatives*** |
|  |  |
| **Chairman** |  |
| Agriculture Machinery Centre, Ministry of Agriculture and Forest  | Mr. Chetem Wangchen |
|  |  |
| **Members** |  |
| Agriculture Machinery Centre, Ministry of Agriculture and Forest  | Mr. Kinga Norbu |
|  |  |
| Agriculture Machinery Centre, Ministry of Agriculture and Forest  | Mr. Sangay Lhendup |
|  |  |
| Construction Development Corporation Limited | Mr. Karma Loday |
|  |  |
| Farm Machinery Corporation Limited, Ministry of Finance  | Mr. Karma Thinley |
|  |  |
| Department of Agriculture, Ministry of Agriculture and Forest | Mr. Tirtha Bdr. Katwal |
| Road Safety and Transport Authority, Ministry of Information and Communication | Mr. Phuntsho Wangdi |
|  |  |
| Technical Training Institute, Samthang, Ministry of Labour and Human Resources | Mr. Sangay Wangchuk |
|  |  |
| Bhutan Standards Bureau, Director General | Mr. Sonam Phuntsho, (Ex- Officio member)  |
|  |  |
| **Member Secretary** |
| Pelden Dendup  |
| Standardization Division, Bhutan Standards Bureau |